Fire door inspection checklist
A fire door register with the routine checks for each doorset: label, closing and latching, hardware, seals, clearances and hold-open devices.
1. Site details
	Building and address
	

	Date of inspection
	

	Inspector and company
	

	Previous register / report reference
	



2. Fire door register
	Door ID
	Level / location
	Type
	Rating on tag
	Result

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



3. Per-door checks
	Check
	Yes
	No
	N/A
	Notes / item IDs

	Compliance tag or label on door leaf and frame, legible
	☐
	☐
	☐
	

	Door closes fully and latches from the fully open position
	☐
	☐
	☐
	

	Self-closer operating, not disconnected or adjusted off
	☐
	☐
	☐
	

	Latch and lock hardware operating, no non-compliant additions
	☐
	☐
	☐
	

	Hinges secure, no missing screws
	☐
	☐
	☐
	

	Clearances around the leaf within the tested doorset’s limits
	☐
	☐
	☐
	

	Smoke seals present and undamaged (smoke doors)
	☐
	☐
	☐
	

	No unauthorised holes, vision panels or modifications
	☐
	☐
	☐
	

	Door not wedged or held open, except by an approved hold-open device
	☐
	☐
	☐
	

	Hold-open device releases on alarm
	☐
	☐
	☐
	

	Required signage present
	☐
	☐
	☐
	



4. Defects and actions
	Door ID
	Defect
	Severity
	Recommended action
	Photo ref

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



5. Summary and sign-off
	Doors inspected / passed / failed
	

	Comments
	

	Inspector name / accreditation / date
	



Free template from SurveyThanks. Fill it in on your phone and generate the report automatically: https://www.surveythanks.com/templates/fire-door-inspection-checklist    Page 
